* Add opamp buffer between Linkwitz filters and speaker outputs.
* 196 ohm resistor exists to prevent short-circuited output from causing damage to filters
* Cable capacitance effects can also be mitigated by 196 ohm